| **Qty** | **Description** | **Price** |
| --- | --- | --- |
| 1 | PATTERSON FPVT ENGINE DRIVEN VERTICAL TURBINE FIRE PUMP |  |
|  | MODEL {model} |  |
|  | {no\_stage} STAGES, {approval} |  |
|  |  |  |
|  | REFERENCE DATA {medium} |  |
|  |  |  |
|  | SPECIFIC GRAVITY (S.G.) {specific\_gravity} |  |
|  |  |  |
|  | RATED CONDITIONS |  |
|  | {capacity} GPM, {discharge\_pressure} DPSI |  |
|  | {rated\_speed} RPM, {pump\_hp} BHP {curve\_details} |  |
|  |  |  |
|  | PRICING VALID UP TILL |  |
|  | {column\_length} FT COLUMN | {column\_price} |
|  |  |  |
|  | PUMP MATERIAL | {pump\_price} |
|  | {pump\_material} |  |
|  |  |  |
|  | COUPLING GUARD {coupling\_guard} |  |
|  |  |  |
|  | BASKET STRAINER {strainer\_material} | {strainer\_price} |
|  |  |  |
|  | MASS ELASTIC TORSIONAL SYSTEM CALCULATION |  |
|  |  |  |
| 1 | {driver\_make} MODEL {driver\_model} | {engine\_price} |
|  | DIESEL ENGINE TIER: {tier} |  |
|  | ARRANGED FOR DUAL BATTERIES |  |
|  | AUTOMATIC OPERATION |  |
|  | RATED FOR {rated\_hp} HP @ {rated\_speed} RPM |  |
|  | WITH HOT START |  |
|  | {engine\_starter} VOLT ENGINE, {single\_power} |  |
|  | {engine\_options} | {engine\_opt\_price} |
| 1 | RIGHT ANGLE GEAR DRIVE |  |
|  | FACTORY CHOICE |  |
|  | {gear\_ratio} GEAR RATIO |  |
|  | {gear\_options} | {gear\_option} |
| 1 | STANDARD FLEXIBLE DRIVE SHAFT, {drive\_shaft} | {driveshaft\_price} |
|  |  |  |
| 1 | STANDARD SHAFT GUARD, {shaft\_guard} | {shaft\_guard\_price} |
|  |  |  |
| 1 | {controller\_make} MODEL {controller\_model} | {controller\_price} |
|  | UL-FM APPROVED |  |
|  | AUTOMATIC ENGINE CONTROLLER FOR |  |
|  | {engine\_starter} VOLT, NEGATIVE GROUND |  |
|  | DUAL BATTERY OPERATION |  |
|  | BUILT IN BATTERY CHARGER |  |
|  | WEEKLY TEST START |  |
|  | {controller\_options} | {controller\_opt\_price} |
|  | ENGINE ACCESSORIES |  |
| {qty\_muff} | MUFFLER {muffler\_options} | {muffler\_price} |
| {qty\_exha} | FLEXIBLE EXHAUST CONNECTOR |  |
| 1 | STANDARD BATTERIES W/ CABLES ({battery\_type}) |  |
| 1 | STANDARD {engine\_starter} VOLT BATTERY RACK | {battery\_rack\_price} |
| 1 | {fuel\_tank\_capacity} GALLON FUEL TANK W/ GAGE | {fuel\_tank\_price} |
|  | {no\_walls} WITH LEGS |  |
| 1 | EMERGENCY VENT VALVE |  |
| 1 | FLEXIBLE FUEL LINES |  |
|  |  |  |
|  | PUMP ACCESSORIES |  |
| 1 | 2” AUTOMATIC AIR RELEASE VALVE, {aarv\_options} | {aarv\_price} |
| 1 | DISCHARGE GAUGE {discharge\_gauge\_options} | {discharge\_gauge\_price} |
| 1 | {mrv\_size} MAIN RELIEF VALVE  {mrv\_options} | {mrv\_price} |
| 1 | ENCLOSED WASTE CONE, {wc\_size} | {wc\_price} |
|  |  |  |
|  | ONE LOT SHIPMENT |  |
|  |  |  |
|  | FOR {packaging\_option} | {packaging\_adder} |
|  | SELL PRICE | {total\_price} |

|  |
| --- |
| **Technical Clarifications / Exceptions** |
| {notes} |

|  |
| --- |
| **Terms & Conditions** |
| We are pleased to offer the following equipment for your consideration on this project. Lead time is subjected to changes (without notice) at the point of order entry. This proposal is based on Patterson Pump Company’s Standard Terms and Conditions of Sale and Patterson Pump Company’s Standard Warranty available at [www.pattersonpumps.com](http://www.pattersonpumps.com). All orders are subject to final review and acceptance of the Contracts Administration Department of Patterson Pump Company. |